Rename the unforce_h9se.txt to force_h9se.txt and move it to the root of your usb-stick
When you enter the recovery menu then it will force to install the image openvix-6.5.002.release-zgemmah92hse_multi.zip in the linux1 selection
